1. Sequence number: 127 + 80 = 207

Source port number: 302

Destination port number: 80

1. Acknowledgement number: 207

Source port number: 80

Destination port number: 302

1. Acknowledgement number: 127 (still waiting for bytes 127 and onwards)

